export const carbonfootprint : CarbonProps[] = [

{

category: 'Weaving Crafts',

subcategory: [

{

name: 'Pashmina Shawl',

RawMaterial: [

{ name: "Pure Pashmina (100%)", value: "2-3 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "4-5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "4-5 kg CO₂" },

{ name: "Synthetic Blend", value: "6-7 kg CO₂" }

],

Processing: [

{

name: "Wool Cleaning",

values: [

{ name: "Pure Pashmina (100%)", value: "1-1 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "1-1.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-2.5 kg CO₂" }

]

},

{

name: "Spinning",

values: [

{ name: "Pure Pashmina (100%)", value: "0.5-1 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "Dyeing (Natural)",

values: [

{ name: "Pure Pashmina (100%)", value: "0.5-0.5 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "0.5-1 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Blend", value: "0-0 kg CO₂" }

]

},

{

name: "Dyeing (Synthetic)",

values: [

{ name: "Pure Pashmina (100%)", value: "0-0 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "1-1.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-2.5 kg CO₂" }

]

}

],

ProductionMethod: [

{

name: "Hand Weaving",

values: [

{ name: "Pure Pashmina (100%)", value: "0.5-1 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "1-1.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "Handloom Weaving",

values: [

{ name: "Pure Pashmina (100%)", value: "1.5-2 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "2-2.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "2-2.5 kg CO₂" },

{ name: "Synthetic Blend", value: "3-4 kg CO₂" }

]

},

{

name: "Mass Production",

values: [

{ name: "Pure Pashmina (100%)", value: "0-0 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "4-6 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "5-6 kg CO₂" },

{ name: "Synthetic Blend", value: "6-7 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic",

values: [

{ name: "Pure Pashmina (100%)", value: "0.5-0.5 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "0.5-1 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Blend", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Papier-Mâché)",

values: [

{ name: "Pure Pashmina (100%)", value: "2-2 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "2-2.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "2-2.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "Plastic",

values: [

{ name: "Pure Pashmina (100%)", value: "1-1.5 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "1-1.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "1-2 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Pure Pashmina (100%)", value: "0.5-1 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "0.5-1.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "0.5-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "1-2 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Pure Pashmina (100%)", value: "1-2 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Pure Pashmina (100%)", value: "5-7 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "5-7 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "5-7 kg CO₂" },

{ name: "Synthetic Blend", value: "6-8 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Pure Pashmina (100%)", value: "2-3 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Blend", value: "3-4 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Pure Pashmina (100%)", value: "1-1 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "1-2 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "1-2 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

}

]

},

{

name: 'Kani Shawl',

RawMaterial: [

{ name: "Pure (Pashmina)", value: "2-3 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "4-5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "4-5 kg CO₂" },

{ name: "Synthetic Blend", value: "6-7 kg CO₂" }

],

Processing: [

{

name: "Wool Cleaning",

values: [

{ name: "Pure (Pashmina)", value: "1-1 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "1-1.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-2.5 kg CO₂" }

]

},

{

name: "Spinning",

values: [

{ name: "Pure (Pashmina)", value: "0.5-1 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "Dyeing (Natural)",

values: [

{ name: "Pure (Pashmina)", value: "0.5-0.5 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "0.5-1 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Blend", value: "0-0 kg CO₂" }

]

},

{

name: "Dyeing (Synthetic)",

values: [

{ name: "Pure (Pashmina)", value: "0-0 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "1-1.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-2.5 kg CO₂" }

]

}

],

Crafting: [

{

name: "Kani Weaving",

values: [

{ name: "Pure (Pashmina)", value: "2-3 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "3-4 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "3-4 kg CO₂" },

{ name: "Synthetic Blend", value: "4-5 kg CO₂" }

]

},

{

name: "Complexity (Simple)",

values: [

{ name: "Pure (Pashmina)", value: "1-1.5 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "1.5-2 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "Complexity (Intricate)",

values: [

{ name: "Pure (Pashmina)", value: "2-3 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Blend", value: "3-4.5 kg CO₂" }

]

},

{

name: "Mass Production",

values: [

{ name: "Pure (Pashmina)", value: "0-0 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "5-6 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "5-6 kg CO₂" },

{ name: "Synthetic Blend", value: "6-7 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic",

values: [

{ name: "Pure (Pashmina)", value: "0.5-0.5 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "0.5-1 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Blend", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Papier-Mâché)",

values: [

{ name: "Pure (Pashmina)", value: "2-2 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "2-2.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "2-2.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "Plastic",

values: [

{ name: "Pure (Pashmina)", value: "1-1.5 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "1-1.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "1-2 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Pure (Pashmina)", value: "0.5-1 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "0.5-1.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "0.5-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "1-2 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Pure (Pashmina)", value: "1-2 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Pure (Pashmina)", value: "5-7 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "5-7 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "5-7 kg CO₂" },

{ name: "Synthetic Blend", value: "6-8 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Pure (Pashmina)", value: "2-3 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Blend", value: "3-4 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Pure (Pashmina)", value: "1-1 kg CO₂" },

{ name: "Pashmina-Silk Blend", value: "1-2 kg CO₂" },

{ name: "Pashmina-Wool Blend", value: "1-2 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

}

]

},

{

name: 'Silk',

RawMaterial: [

{ name: "Pure Silk", value: "4-6 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "3-5 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "3-4 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "5-7 kg CO₂" }

],

Processing: [

{

name: "Sericulture (Mulberry Farming)",

values: [

{ name: "Pure Silk", value: "2-3 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "1-2 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "1-2 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "0-0 kg CO₂" }

]

},

{

name: "Spinning",

values: [

{ name: "Pure Silk", value: "1-1.5 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "1.5-2 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "2-2.5 kg CO₂" }

]

},

{

name: "Dyeing (Natural)",

values: [

{ name: "Pure Silk", value: "0.5-1 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "0.5-1 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "0-0 kg CO₂" }

]

},

{

name: "Dyeing (Synthetic)",

values: [

{ name: "Pure Silk", value: "0-0 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "1-1.5 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "2-3 kg CO₂" }

]

}

],

Crafting: [

{

name: "Handloom Weaving",

values: [

{ name: "Pure Silk", value: "1-2 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "2-3 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "3-4 kg CO₂" }

]

},

{

name: "Machine Weaving",

values: [

{ name: "Pure Silk", value: "2-3 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "3-4 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "4-5 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic",

values: [

{ name: "Pure Silk", value: "0.5-0.5 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "0.5-1 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Papier-Mâché)",

values: [

{ name: "Pure Silk", value: "2-3 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "2-2.5 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "2-2.5 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "2-3 kg CO₂" }

]

},

{

name: "Plastic",

values: [

{ name: "Pure Silk", value: "1-1.5 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "1-1.5 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "1-2 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Pure Silk", value: "0.5-1 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "0.5-1.5 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "0.5-1.5 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "1-2 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Pure Silk", value: "1-2 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "2-3 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Pure Silk", value: "5-7 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "5-7 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "5-7 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "6-8 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Pure Silk", value: "2-3 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "3-4 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Pure Silk", value: "1-1 kg CO₂" },

{ name: "Silk-Pashmina Blend", value: "1-2 kg CO₂" },

{ name: "Silk-Cotton Blend", value: "1-2 kg CO₂" },

{ name: "Synthetic Silk Blend", value: "2-3 kg CO₂" }

]

}

]

},

{

name: 'Carpet',

RawMaterial: [

{ name: "Silk on Silk", value: "5-7 kg CO₂" },

{ name: "Silk on Cotton", value: "4-6 kg CO₂" },

{ name: "Cotton on Cotton", value: "3-4 kg CO₂" },

{ name: "Cotton on Wool", value: "4-5 kg CO₂" },

{ name: "Synthetic Blend", value: "6-8 kg CO₂" }

],

Processing: [

{

name: "Material Cleaning",

values: [

{ name: "Silk on Silk", value: "1.5-2 kg CO₂" },

{ name: "Silk on Cotton", value: "1-1.5 kg CO₂" },

{ name: "Cotton on Cotton", value: "1-1.5 kg CO₂" },

{ name: "Cotton on Wool", value: "1-2 kg CO₂" },

{ name: "Synthetic Blend", value: "2-2.5 kg CO₂" }

]

},

{

name: "Spinning",

values: [

{ name: "Silk on Silk", value: "2-3 kg CO₂" },

{ name: "Silk on Cotton", value: "1.5-2.5 kg CO₂" },

{ name: "Cotton on Cotton", value: "1-1.5 kg CO₂" },

{ name: "Cotton on Wool", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "Dyeing (Natural)",

values: [

{ name: "Silk on Silk", value: "1-1.5 kg CO₂" },

{ name: "Silk on Cotton", value: "0.5-1 kg CO₂" },

{ name: "Cotton on Cotton", value: "0.5-1 kg CO₂" },

{ name: "Cotton on Wool", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Blend", value: "0-0 kg CO₂" }

]

},

{

name: "Dyeing (Synthetic)",

values: [

{ name: "Silk on Silk", value: "0-0 kg CO₂" },

{ name: "Silk on Cotton", value: "1-1.5 kg CO₂" },

{ name: "Cotton on Cotton", value: "1-1.5 kg CO₂" },

{ name: "Cotton on Wool", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand-Knotting (Simple)",

values: [

{ name: "Silk on Silk", value: "4-5 kg CO₂" },

{ name: "Silk on Cotton", value: "3-4 kg CO₂" },

{ name: "Cotton on Cotton", value: "2-3 kg CO₂" },

{ name: "Cotton on Wool", value: "3-4 kg CO₂" },

{ name: "Synthetic Blend", value: "5-6 kg CO₂" }

]

},

{

name: "Hand-Knotting (Intricate)",

values: [

{ name: "Silk on Silk", value: "6-8 kg CO₂" },

{ name: "Silk on Cotton", value: "5-6 kg CO₂" },

{ name: "Cotton on Cotton", value: "4-5 kg CO₂" },

{ name: "Cotton on Wool", value: "5-6 kg CO₂" },

{ name: "Synthetic Blend", value: "7-9 kg CO₂" }

]

},

{

name: "Machine-Knotting (Mass Production)",

values: [

{ name: "Silk on Silk", value: "8-10 kg CO₂" },

{ name: "Silk on Cotton", value: "7-8 kg CO₂" },

{ name: "Cotton on Cotton", value: "6-7 kg CO₂" },

{ name: "Cotton on Wool", value: "7-8 kg CO₂" },

{ name: "Synthetic Blend", value: "9-10 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic",

values: [

{ name: "Silk on Silk", value: "1-1.5 kg CO₂" },

{ name: "Silk on Cotton", value: "0.5-1 kg CO₂" },

{ name: "Cotton on Cotton", value: "0.5-1 kg CO₂" },

{ name: "Cotton on Wool", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Blend", value: "1-2 kg CO₂" }

]

},

{

name: "Luxury (Papier-Mâché)",

values: [

{ name: "Silk on Silk", value: "2-3 kg CO₂" },

{ name: "Silk on Cotton", value: "2-2.5 kg CO₂" },

{ name: "Cotton on Cotton", value: "2-2.5 kg CO₂" },

{ name: "Cotton on Wool", value: "2-2.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Silk on Silk", value: "1-2 kg CO₂" },

{ name: "Silk on Cotton", value: "1-1.5 kg CO₂" },

{ name: "Cotton on Cotton", value: "0.5-1 kg CO₂" },

{ name: "Cotton on Wool", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Silk on Silk", value: "2-3 kg CO₂" },

{ name: "Silk on Cotton", value: "1.5-2.5 kg CO₂" },

{ name: "Cotton on Cotton", value: "1-2 kg CO₂" },

{ name: "Cotton on Wool", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Blend", value: "3-4 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Silk on Silk", value: "6-8 kg CO₂" },

{ name: "Silk on Cotton", value: "5-7 kg CO₂" },

{ name: "Cotton on Cotton", value: "5-6 kg CO₂" },

{ name: "Cotton on Wool", value: "5-7 kg CO₂" },

{ name: "Synthetic Blend", value: "8-10 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Silk on Silk", value: "3-5 kg CO₂" },

{ name: "Silk on Cotton", value: "2.5-4 kg CO₂" },

{ name: "Cotton on Cotton", value: "2-3.5 kg CO₂" },

{ name: "Cotton on Wool", value: "2.5-4 kg CO₂" },

{ name: "Synthetic Blend", value: "5-7 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Silk on Silk", value: "1.5-2.5 kg CO₂" },

{ name: "Silk on Cotton", value: "1-2 kg CO₂" },

{ name: "Cotton on Cotton", value: "0.5-1.5 kg CO₂" },

{ name: "Cotton on Wool", value: "1-2 kg CO₂" },

{ name: "Synthetic Blend", value: "2.5-3.5 kg CO₂" }

]

}

]

},

]

},

{

category: 'Embroidery Craft',

subcategory: [

{

name: 'Embroidery craft',

RawMaterial: [

{ name: "Pure Cotton Base", value: "2-3 kg CO₂" },

{ name: "Silk Base", value: "3-4 kg CO₂" },

{ name: "Wool Base", value: "4-5 kg CO₂" },

{ name: "Synthetic Base", value: "5-7 kg CO₂" }

],

Processing: [

{

name: "Base Preparation (Manual)",

values: [

{ name: "Pure Cotton Base", value: "0.5-1 kg CO₂" },

{ name: "Silk Base", value: "1-1.5 kg CO₂" },

{ name: "Wool Base", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Base", value: "0-0 kg CO₂" }

]

},

{

name: "Base Preparation (Machine)",

values: [

{ name: "Pure Cotton Base", value: "1-1.5 kg CO₂" },

{ name: "Silk Base", value: "1.5-2 kg CO₂" },

{ name: "Wool Base", value: "2-3 kg CO₂" },

{ name: "Synthetic Base", value: "3-4 kg CO₂" }

]

}

],

Crafting: [

{

name: "Sozni Embroidery (Simple)",

values: [

{ name: "Pure Cotton Base", value: "2-3 kg CO₂" },

{ name: "Silk Base", value: "2.5-3.5 kg CO₂" },

{ name: "Wool Base", value: "3-4 kg CO₂" },

{ name: "Synthetic Base", value: "4-5 kg CO₂" }

]

},

{

name: "Sozni Embroidery (Intricate)",

values: [

{ name: "Pure Cotton Base", value: "3-4 kg CO₂" },

{ name: "Silk Base", value: "3.5-4.5 kg CO₂" },

{ name: "Wool Base", value: "4-5 kg CO₂" },

{ name: "Synthetic Base", value: "5-6 kg CO₂" }

]

},

{

name: "Aari Work (Simple)",

values: [

{ name: "Pure Cotton Base", value: "1-2 kg CO₂" },

{ name: "Silk Base", value: "2-3 kg CO₂" },

{ name: "Wool Base", value: "3-4 kg CO₂" },

{ name: "Synthetic Base", value: "4-5 kg CO₂" }

]

},

{

name: "Aari Work (Intricate)",

values: [

{ name: "Pure Cotton Base", value: "2-3 kg CO₂" },

{ name: "Silk Base", value: "3-4 kg CO₂" },

{ name: "Wool Base", value: "4-5 kg CO₂" },

{ name: "Synthetic Base", value: "5-6 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Paper/Cloth)",

values: [

{ name: "Pure Cotton Base", value: "0.5 kg CO₂" },

{ name: "Silk Base", value: "0.5-1 kg CO₂" },

{ name: "Wool Base", value: "1 kg CO₂" },

{ name: "Synthetic Base", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly)",

values: [

{ name: "Pure Cotton Base", value: "1-1.5 kg CO₂" },

{ name: "Silk Base", value: "1-2 kg CO₂" },

{ name: "Wool Base", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Base", value: "2-3 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Pure Cotton Base", value: "0.5-1 kg CO₂" },

{ name: "Silk Base", value: "1-1.5 kg CO₂" },

{ name: "Wool Base", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Base", value: "2-3 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Pure Cotton Base", value: "1-2 kg CO₂" },

{ name: "Silk Base", value: "2-3 kg CO₂" },

{ name: "Wool Base", value: "3-4 kg CO₂" },

{ name: "Synthetic Base", value: "4-5 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Pure Cotton Base", value: "3-5 kg CO₂" },

{ name: "Silk Base", value: "5-6 kg CO₂" },

{ name: "Wool Base", value: "6-8 kg CO₂" },

{ name: "Synthetic Base", value: "7-9 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Pure Cotton Base", value: "1.5-3 kg CO₂" },

{ name: "Silk Base", value: "2.5-4 kg CO₂" },

{ name: "Wool Base", value: "3.5-5 kg CO₂" },

{ name: "Synthetic Base", value: "4.5-6 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Pure Cotton Base", value: "1-1.5 kg CO₂" },

{ name: "Silk Base", value: "1.5-2 kg CO₂" },

{ name: "Wool Base", value: "2-3 kg CO₂" },

{ name: "Synthetic Base", value: "2.5-4 kg CO₂" }

]

}

]

}

]

},

{

category: 'Wood Crafts',

subcategory: [

{

name: 'Walnut Wood Carving Furniture',

RawMaterial: [

{ name: "Pure Walnut Wood", value: "5-7 kg CO₂" },

{ name: "Walnut with MDF Base", value: "4-6 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "6-9 kg CO₂" }

],

Processing: [

{

name: "Wood Harvesting",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3.5 kg CO₂" }

]

},

{

name: "Drying (Natural)",

values: [

{ name: "Pure Walnut Wood", value: "1-1.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "0-0 kg CO₂" }

]

},

{

name: "Drying (Kiln)",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3 kg CO₂" }

]

},

{

name: "Surface Finishing (Manual)",

values: [

{ name: "Pure Walnut Wood", value: "0.5-1 kg CO₂" },

{ name: "Walnut with MDF Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "0-0 kg CO₂" }

]

},

{

name: "Surface Finishing (Machine)",

values: [

{ name: "Pure Walnut Wood", value: "0-0 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "1.5-2 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand Carving (Simple)",

values: [

{ name: "Pure Walnut Wood", value: "3-4 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2-3 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "3-4 kg CO₂" }

]

},

{

name: "Hand Carving (Intricate)",

values: [

{ name: "Pure Walnut Wood", value: "5-6 kg CO₂" },

{ name: "Walnut with MDF Base", value: "4-5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "5-6 kg CO₂" }

]

},

{

name: "Machine-Assisted Carving",

values: [

{ name: "Pure Walnut Wood", value: "4-5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "3-4 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "4-5 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Cardboard)",

values: [

{ name: "Pure Walnut Wood", value: "1-1 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Wooden Box)",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2-3 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Pure Walnut Wood", value: "1-2 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "3-4 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Pure Walnut Wood", value: "6-8 kg CO₂" },

{ name: "Walnut with MDF Base", value: "7-9 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "8-10 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Pure Walnut Wood", value: "3-5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "4-6 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "5-7 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Pure Walnut Wood", value: "1.5-2.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2-3 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2.5-3.5 kg CO₂" }

]

}

]

},

{

name: 'Khatamband',

RawMaterial: [

{ name: "Pure Walnut Wood", value: "5-7 kg CO₂" },

{ name: "Walnut with MDF Base", value: "4-6 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "6-8 kg CO₂" }

],

Processing: [

{

name: "Wood Harvesting",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3.5 kg CO₂" }

]

},

{

name: "Drying (Natural)",

values: [

{ name: "Pure Walnut Wood", value: "1-1.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "0-0 kg CO₂" }

]

},

{

name: "Drying (Kiln)",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3 kg CO₂" }

]

},

{

name: "Surface Finishing (Manual)",

values: [

{ name: "Pure Walnut Wood", value: "0.5-1 kg CO₂" },

{ name: "Walnut with MDF Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "0-0 kg CO₂" }

]

},

{

name: "Surface Finishing (Machine)",

values: [

{ name: "Pure Walnut Wood", value: "0-0 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "1.5-2 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand Assembly (Simple Patterns)",

values: [

{ name: "Pure Walnut Wood", value: "3-4 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2-3 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "3-4 kg CO₂" }

]

},

{

name: "Hand Assembly (Intricate Patterns)",

values: [

{ name: "Pure Walnut Wood", value: "5-6 kg CO₂" },

{ name: "Walnut with MDF Base", value: "4-5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "5-6 kg CO₂" }

]

},

{

name: "Machine-Assisted Assembly",

values: [

{ name: "Pure Walnut Wood", value: "4-5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "3-4 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "4-5 kg CO₂" }

]

}

],

Installation: [

{

name: "Local Installation",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3 kg CO₂" }

]

},

{

name: "Remote Installation",

values: [

{ name: "Pure Walnut Wood", value: "3-5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2.5-4 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "3.5-5 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Cardboard)",

values: [

{ name: "Pure Walnut Wood", value: "1-1 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Wooden Box)",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2-3 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Pure Walnut Wood", value: "1-2 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "3-4 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Pure Walnut Wood", value: "6-8 kg CO₂" },

{ name: "Walnut with MDF Base", value: "7-9 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "8-10 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Pure Walnut Wood", value: "3-5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "4-6 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "5-7 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Pure Walnut Wood", value: "1.5-2.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2-3 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2.5-3.5 kg CO₂" }

]

}

]

},

{

name: 'Pinjrakari',

RawMaterial: [

{ name: "Pure Walnut Wood", value: "5-7 kg CO₂" },

{ name: "Walnut with MDF Base", value: "4-6 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "6-8 kg CO₂" }

],

Processing: [

{

name: "Wood Harvesting",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3.5 kg CO₂" }

]

},

{

name: "Drying (Natural)",

values: [

{ name: "Pure Walnut Wood", value: "1-1.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "0-0 kg CO₂" }

]

},

{

name: "Drying (Kiln)",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3 kg CO₂" }

]

},

{

name: "Surface Finishing (Manual)",

values: [

{ name: "Pure Walnut Wood", value: "0.5-1 kg CO₂" },

{ name: "Walnut with MDF Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "0-0 kg CO₂" }

]

},

{

name: "Surface Finishing (Machine)",

values: [

{ name: "Pure Walnut Wood", value: "0-0 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "1.5-2 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand Assembly (Simple Patterns)",

values: [

{ name: "Pure Walnut Wood", value: "3-4 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2-3 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "3-4 kg CO₂" }

]

},

{

name: "Hand Assembly (Intricate Patterns)",

values: [

{ name: "Pure Walnut Wood", value: "5-6 kg CO₂" },

{ name: "Walnut with MDF Base", value: "4-5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "5-6 kg CO₂" }

]

},

{

name: "Machine-Assisted Assembly",

values: [

{ name: "Pure Walnut Wood", value: "4-5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "3-4 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "4-5 kg CO₂" }

]

}

],

Installation: [

{

name: "Local Installation",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3 kg CO₂" }

]

},

{

name: "Remote Installation",

values: [

{ name: "Pure Walnut Wood", value: "3-5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2.5-4 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "3.5-5 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Cardboard)",

values: [

{ name: "Pure Walnut Wood", value: "1-1 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Wooden Box)",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2-3 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Pure Walnut Wood", value: "1-2 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "3-4 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Pure Walnut Wood", value: "6-8 kg CO₂" },

{ name: "Walnut with MDF Base", value: "7-9 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "8-10 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Pure Walnut Wood", value: "3-5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "4-6 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "5-7 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Pure Walnut Wood", value: "1.5-2.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2-3 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2.5-3.5 kg CO₂" }

]

}

]

},

{

name: 'Wicker Work',

RawMaterial: [

{ name: "Pure Willow Wicker", value: "2-3 kg CO₂" },

{ name: "Willow with Bamboo Base", value: "3-4 kg CO₂" },

{ name: "Synthetic Wicker", value: "4-6 kg CO₂" }

],

Processing: [

{

name: "Harvesting Willow/Bamboo",

values: [

{ name: "Pure Willow Wicker", value: "1-1.5 kg CO₂" },

{ name: "Willow with Bamboo Base", value: "1-2 kg CO₂" },

{ name: "Synthetic Wicker", value: "0-0 kg CO₂" }

]

},

{

name: "Treatment (Natural)",

values: [

{ name: "Pure Willow Wicker", value: "0.5-1 kg CO₂" },

{ name: "Willow with Bamboo Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Wicker", value: "0-0 kg CO₂" }

]

},

{

name: "Treatment (Chemical)",

values: [

{ name: "Pure Willow Wicker", value: "0-0 kg CO₂" },

{ name: "Willow with Bamboo Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Wicker", value: "2-3 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand Weaving (Simple)",

values: [

{ name: "Pure Willow Wicker", value: "1-2 kg CO₂" },

{ name: "Willow with Bamboo Base", value: "2-3 kg CO₂" },

{ name: "Synthetic Wicker", value: "3-4 kg CO₂" }

]

},

{

name: "Hand Weaving (Intricate)",

values: [

{ name: "Pure Willow Wicker", value: "2-3 kg CO₂" },

{ name: "Willow with Bamboo Base", value: "3-4 kg CO₂" },

{ name: "Synthetic Wicker", value: "4-5 kg CO₂" }

]

},

{

name: "Machine-Assisted Weaving",

values: [

{ name: "Pure Willow Wicker", value: "3-4 kg CO₂" },

{ name: "Willow with Bamboo Base", value: "4-5 kg CO₂" },

{ name: "Synthetic Wicker", value: "5-6 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Cardboard)",

values: [

{ name: "Pure Willow Wicker", value: "0.5-0.5 kg CO₂" },

{ name: "Willow with Bamboo Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Wicker", value: "1-1 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly Packaging)",

values: [

{ name: "Pure Willow Wicker", value: "1-1.5 kg CO₂" },

{ name: "Willow with Bamboo Base", value: "1-2 kg CO₂" },

{ name: "Synthetic Wicker", value: "1.5-2 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Pure Willow Wicker", value: "0.5-1 kg CO₂" },

{ name: "Willow with Bamboo Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Wicker", value: "1.5-2 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Pure Willow Wicker", value: "1-2 kg CO₂" },

{ name: "Willow with Bamboo Base", value: "2-3 kg CO₂" },

{ name: "Synthetic Wicker", value: "3-4 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Pure Willow Wicker", value: "3-5 kg CO₂" },

{ name: "Willow with Bamboo Base", value: "5-6 kg CO₂" },

{ name: "Synthetic Wicker", value: "6-8 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Pure Willow Wicker", value: "1.5-3 kg CO₂" },

{ name: "Willow with Bamboo Base", value: "2-3.5 kg CO₂" },

{ name: "Synthetic Wicker", value: "3-5 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Pure Willow Wicker", value: "1-1.5 kg CO₂" },

{ name: "Willow with Bamboo Base", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Wicker", value: "2-3 kg CO₂" }

]

}

]

},

{

name: 'Woodenware Walnut',

RawMaterial: [

{ name: "Pure Walnut Wood", value: "5-7 kg CO₂" },

{ name: "Walnut with MDF Base", value: "4-6 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "6-8 kg CO₂" }

],

Processing: [

{

name: "Wood Harvesting",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3.5 kg CO₂" }

]

},

{

name: "Drying (Natural)",

values: [

{ name: "Pure Walnut Wood", value: "1-1.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "0-0 kg CO₂" }

]

},

{

name: "Drying (Kiln)",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3 kg CO₂" }

]

},

{

name: "Surface Finishing (Manual)",

values: [

{ name: "Pure Walnut Wood", value: "0.5-1 kg CO₂" },

{ name: "Walnut with MDF Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "0-0 kg CO₂" }

]

},

{

name: "Surface Finishing (Machine)",

values: [

{ name: "Pure Walnut Wood", value: "0-0 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "1.5-2 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand Carving (Simple)",

values: [

{ name: "Pure Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2-3 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "3-4 kg CO₂" }

]

},

{

name: "Hand Carving (Intricate)",

values: [

{ name: "Pure Walnut Wood", value: "3-4 kg CO₂" },

{ name: "Walnut with MDF Base", value: "3-4 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "4-5 kg CO₂" }

]

},

{

name: "Machine-Assisted Carving",

values: [

{ name: "Pure Walnut Wood", value: "4-5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "4-5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "5-6 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Cardboard)",

values: [

{ name: "Pure Walnut Wood", value: "0.5-0.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "1-1 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly Packaging)",

values: [

{ name: "Pure Walnut Wood", value: "1-1.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1-2 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "1.5-2 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Pure Walnut Wood", value: "0.5-1 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "1.5-2 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Pure Walnut Wood", value: "1-2 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2-3 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "3-4 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Pure Walnut Wood", value: "6-8 kg CO₂" },

{ name: "Walnut with MDF Base", value: "7-9 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "8-10 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Pure Walnut Wood", value: "3-5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "4-6 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "5-7 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Pure Walnut Wood", value: "1-1.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2 kg CO₂" },

{ name: "Synthetic/Composite Wood", value: "2-3 kg CO₂" }

]

}

]

}

]

},

{

category: 'Decor Crafts',

subcategory: [

{

name: 'Engraved Metalware',

RawMaterial: [

{ name: "Copper Base", value: "5-6 kg CO₂" },

{ name: "Brass Base", value: "4-5 kg CO₂" },

{ name: "Bronze Base", value: "6-7 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "3-4 kg CO₂" }

],

Processing: [

{

name: "Smelting (Manual)",

values: [

{ name: "Copper Base", value: "2-3 kg CO₂" },

{ name: "Brass Base", value: "1.5-2.5 kg CO₂" },

{ name: "Bronze Base", value: "2-3 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "0-0 kg CO₂" }

]

},

{

name: "Smelting (Industrial)",

values: [

{ name: "Copper Base", value: "3-4 kg CO₂" },

{ name: "Brass Base", value: "2-3 kg CO₂" },

{ name: "Bronze Base", value: "3-4 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "1-2 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand Engraving (Simple)",

values: [

{ name: "Copper Base", value: "3-4 kg CO₂" },

{ name: "Brass Base", value: "2-3 kg CO₂" },

{ name: "Bronze Base", value: "3-4 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "2-3 kg CO₂" }

]

},

{

name: "Hand Engraving (Intricate)",

values: [

{ name: "Copper Base", value: "5-6 kg CO₂" },

{ name: "Brass Base", value: "4-5 kg CO₂" },

{ name: "Bronze Base", value: "5-6 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "4-5 kg CO₂" }

]

},

{

name: "Machine-Assisted Engraving",

values: [

{ name: "Copper Base", value: "4-5 kg CO₂" },

{ name: "Brass Base", value: "3-4 kg CO₂" },

{ name: "Bronze Base", value: "4-5 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "3-4 kg CO₂" }

]

}

],

Finishing: [

{

name: "Polishing (Manual)",

values: [

{ name: "Copper Base", value: "1-2 kg CO₂" },

{ name: "Brass Base", value: "1-1.5 kg CO₂" },

{ name: "Bronze Base", value: "1.5-2 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "1-1.5 kg CO₂" }

]

},

{

name: "Polishing (Machine)",

values: [

{ name: "Copper Base", value: "2-3 kg CO₂" },

{ name: "Brass Base", value: "2-2.5 kg CO₂" },

{ name: "Bronze Base", value: "2.5-3 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "1.5-2 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Cardboard)",

values: [

{ name: "Copper Base", value: "0.5-1 kg CO₂" },

{ name: "Brass Base", value: "0.5-1 kg CO₂" },

{ name: "Bronze Base", value: "1 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly Packaging)",

values: [

{ name: "Copper Base", value: "1-1.5 kg CO₂" },

{ name: "Brass Base", value: "1-1.5 kg CO₂" },

{ name: "Bronze Base", value: "1.5-2 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "1.5-2 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Copper Base", value: "0.5-1 kg CO₂" },

{ name: "Brass Base", value: "0.5-1 kg CO₂" },

{ name: "Bronze Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "1.5-2 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Copper Base", value: "1-2 kg CO₂" },

{ name: "Brass Base", value: "1.5-2.5 kg CO₂" },

{ name: "Bronze Base", value: "2-3 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "3-4 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Copper Base", value: "4-6 kg CO₂" },

{ name: "Brass Base", value: "5-7 kg CO₂" },

{ name: "Bronze Base", value: "6-8 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "7-9 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Copper Base", value: "2.5-4 kg CO₂" },

{ name: "Brass Base", value: "3.5-5 kg CO₂" },

{ name: "Bronze Base", value: "4.5-6 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "5.5-7 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Copper Base", value: "1-2 kg CO₂" },

{ name: "Brass Base", value: "1.5-2.5 kg CO₂" },

{ name: "Bronze Base", value: "2-3 kg CO₂" },

{ name: "Synthetic/Alloy Base", value: "2.5-4 kg CO₂" }

]

}

]

},

{

name: 'Tapestry & Chainstitch',

RawMaterial: [

{ name: "Pure Wool Base", value: "3-4 kg CO₂" },

{ name: "Cotton Base", value: "2-3 kg CO₂" },

{ name: "Silk Base", value: "4-5 kg CO₂" },

{ name: "Synthetic Base", value: "5-6 kg CO₂" }

],

Processing: [

{

name: "Base Preparation (Manual)",

values: [

{ name: "Pure Wool Base", value: "0.5-1 kg CO₂" },

{ name: "Cotton Base", value: "0.5-1 kg CO₂" },

{ name: "Silk Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Base", value: "0-0 kg CO₂" }

]

},

{

name: "Base Preparation (Machine)",

values: [

{ name: "Pure Wool Base", value: "1-1.5 kg CO₂" },

{ name: "Cotton Base", value: "1-1.5 kg CO₂" },

{ name: "Silk Base", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Base", value: "2-3 kg CO₂" }

]

}

],

Crafting: [

{

name: "Chainstitch Embroidery (Simple)",

values: [

{ name: "Pure Wool Base", value: "2-3 kg CO₂" },

{ name: "Cotton Base", value: "1.5-2.5 kg CO₂" },

{ name: "Silk Base", value: "2-3 kg CO₂" },

{ name: "Synthetic Base", value: "3-4 kg CO₂" }

]

},

{

name: "Chainstitch Embroidery (Intricate)",

values: [

{ name: "Pure Wool Base", value: "3-4 kg CO₂" },

{ name: "Cotton Base", value: "2.5-3.5 kg CO₂" },

{ name: "Silk Base", value: "3-4 kg CO₂" },

{ name: "Synthetic Base", value: "4-5 kg CO₂" }

]

},

{

name: "Machine-Assisted Chainstitch",

values: [

{ name: "Pure Wool Base", value: "4-5 kg CO₂" },

{ name: "Cotton Base", value: "3-4 kg CO₂" },

{ name: "Silk Base", value: "4-5 kg CO₂" },

{ name: "Synthetic Base", value: "5-6 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Paper/Cloth)",

values: [

{ name: "Pure Wool Base", value: "0.5-1 kg CO₂" },

{ name: "Cotton Base", value: "0.5-1 kg CO₂" },

{ name: "Silk Base", value: "1 kg CO₂" },

{ name: "Synthetic Base", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly)",

values: [

{ name: "Pure Wool Base", value: "1-1.5 kg CO₂" },

{ name: "Cotton Base", value: "1-1.5 kg CO₂" },

{ name: "Silk Base", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Base", value: "2-3 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Pure Wool Base", value: "0.5-1 kg CO₂" },

{ name: "Cotton Base", value: "0.5-1 kg CO₂" },

{ name: "Silk Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Base", value: "1.5-2 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Pure Wool Base", value: "1-2 kg CO₂" },

{ name: "Cotton Base", value: "1.5-2.5 kg CO₂" },

{ name: "Silk Base", value: "2-3 kg CO₂" },

{ name: "Synthetic Base", value: "3-4 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Pure Wool Base", value: "4-5 kg CO₂" },

{ name: "Cotton Base", value: "5-6 kg CO₂" },

{ name: "Silk Base", value: "6-7 kg CO₂" },

{ name: "Synthetic Base", value: "7-8 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Pure Wool Base", value: "2.5-4 kg CO₂" },

{ name: "Cotton Base", value: "3-4.5 kg CO₂" },

{ name: "Silk Base", value: "4-5.5 kg CO₂" },

{ name: "Synthetic Base", value: "5-6.5 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Pure Wool Base", value: "1-1.5 kg CO₂" },

{ name: "Cotton Base", value: "1.5-2 kg CO₂" },

{ name: "Silk Base", value: "2-3 kg CO₂" },

{ name: "Synthetic Base", value: "2.5-3.5 kg CO₂" }

]

}

]

},

{

name: 'Crewel Work',

RawMaterial: [

{ name: "Wool Base", value: "3-4 kg CO₂" },

{ name: "Cotton Base", value: "2-3 kg CO₂" },

{ name: "Silk Base", value: "4-5 kg CO₂" },

{ name: "Synthetic Base", value: "5-6 kg CO₂" }

],

Processing: [

{

name: "Base Preparation (Manual)",

values: [

{ name: "Wool Base", value: "0.5-1 kg CO₂" },

{ name: "Cotton Base", value: "0.5-1 kg CO₂" },

{ name: "Silk Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Base", value: "0-0 kg CO₂" }

]

},

{

name: "Base Preparation (Machine)",

values: [

{ name: "Wool Base", value: "1-1.5 kg CO₂" },

{ name: "Cotton Base", value: "1-1.5 kg CO₂" },

{ name: "Silk Base", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Base", value: "2-3 kg CO₂" }

]

}

],

Crafting: [

{

name: "Crewel Embroidery (Simple)",

values: [

{ name: "Wool Base", value: "2-3 kg CO₂" },

{ name: "Cotton Base", value: "1.5-2.5 kg CO₂" },

{ name: "Silk Base", value: "2-3 kg CO₂" },

{ name: "Synthetic Base", value: "3-4 kg CO₂" }

]

},

{

name: "Crewel Embroidery (Intricate)",

values: [

{ name: "Wool Base", value: "3-4 kg CO₂" },

{ name: "Cotton Base", value: "2.5-3.5 kg CO₂" },

{ name: "Silk Base", value: "3-4 kg CO₂" },

{ name: "Synthetic Base", value: "4-5 kg CO₂" }

]

},

{

name: "Machine-Assisted Crewel Work",

values: [

{ name: "Wool Base", value: "4-5 kg CO₂" },

{ name: "Cotton Base", value: "3-4 kg CO₂" },

{ name: "Silk Base", value: "4-5 kg CO₂" },

{ name: "Synthetic Base", value: "5-6 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Paper/Cloth)",

values: [

{ name: "Wool Base", value: "0.5-1 kg CO₂" },

{ name: "Cotton Base", value: "0.5-1 kg CO₂" },

{ name: "Silk Base", value: "1 kg CO₂" },

{ name: "Synthetic Base", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly)",

values: [

{ name: "Wool Base", value: "1-1.5 kg CO₂" },

{ name: "Cotton Base", value: "1-1.5 kg CO₂" },

{ name: "Silk Base", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Base", value: "2-3 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Wool Base", value: "0.5-1 kg CO₂" },

{ name: "Cotton Base", value: "0.5-1 kg CO₂" },

{ name: "Silk Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Base", value: "1.5-2 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Wool Base", value: "1-2 kg CO₂" },

{ name: "Cotton Base", value: "1.5-2.5 kg CO₂" },

{ name: "Silk Base", value: "2-3 kg CO₂" },

{ name: "Synthetic Base", value: "3-4 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Wool Base", value: "4-5 kg CO₂" },

{ name: "Cotton Base", value: "5-6 kg CO₂" },

{ name: "Silk Base", value: "6-7 kg CO₂" },

{ name: "Synthetic Base", value: "7-8 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Wool Base", value: "2.5-4 kg CO₂" },

{ name: "Cotton Base", value: "3-4.5 kg CO₂" },

{ name: "Silk Base", value: "4-5.5 kg CO₂" },

{ name: "Synthetic Base", value: "5-6.5 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Wool Base", value: "1-1.5 kg CO₂" },

{ name: "Cotton Base", value: "1.5-2 kg CO₂" },

{ name: "Silk Base", value: "2-3 kg CO₂" },

{ name: "Synthetic Base", value: "2.5-3.5 kg CO₂" }

]

}

]

},

{

name: "Silverware Craft",

RawMaterial: [

{ name: "Pure Silver", value: "6-8 kg CO₂" },

{ name: "Silver Alloy", value: "4-6 kg CO₂" },

{ name: "Plated Silver", value: "3-5 kg CO₂" }

],

Processing: [

{

name: "Smelting (Manual)",

values: [

{ name: "Pure Silver", value: "3-4 kg CO₂" },

{ name: "Silver Alloy", value: "2-3 kg CO₂" },

{ name: "Plated Silver", value: "1-2 kg CO₂" }

]

},

{

name: "Smelting (Industrial)",

values: [

{ name: "Pure Silver", value: "4-5 kg CO₂" },

{ name: "Silver Alloy", value: "3-4 kg CO₂" },

{ name: "Plated Silver", value: "2-3 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand Engraving (Simple)",

values: [

{ name: "Pure Silver", value: "3-4 kg CO₂" },

{ name: "Silver Alloy", value: "2.5-3.5 kg CO₂" },

{ name: "Plated Silver", value: "2-3 kg CO₂" }

]

},

{

name: "Hand Engraving (Intricate)",

values: [

{ name: "Pure Silver", value: "5-6 kg CO₂" },

{ name: "Silver Alloy", value: "4-5 kg CO₂" },

{ name: "Plated Silver", value: "3-4 kg CO₂" }

]

},

{

name: "Machine-Assisted Engraving",

values: [

{ name: "Pure Silver", value: "4-5 kg CO₂" },

{ name: "Silver Alloy", value: "3.5-4.5 kg CO₂" },

{ name: "Plated Silver", value: "3-4 kg CO₂" }

]

}

],

Finishing: [

{

name: "Polishing (Manual)",

values: [

{ name: "Pure Silver", value: "1-2 kg CO₂" },

{ name: "Silver Alloy", value: "1-1.5 kg CO₂" },

{ name: "Plated Silver", value: "0.5-1 kg CO₂" }

]

},

{

name: "Polishing (Machine)",

values: [

{ name: "Pure Silver", value: "2-3 kg CO₂" },

{ name: "Silver Alloy", value: "1.5-2.5 kg CO₂" },

{ name: "Plated Silver", value: "1-1.5 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Cardboard)",

values: [

{ name: "Pure Silver", value: "0.5-1 kg CO₂" },

{ name: "Silver Alloy", value: "0.5-1 kg CO₂" },

{ name: "Plated Silver", value: "0.5-1 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly Packaging)",

values: [

{ name: "Pure Silver", value: "1-1.5 kg CO₂" },

{ name: "Silver Alloy", value: "1-1.5 kg CO₂" },

{ name: "Plated Silver", value: "1-1.5 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Pure Silver", value: "0.5-1 kg CO₂" },

{ name: "Silver Alloy", value: "0.5-1 kg CO₂" },

{ name: "Plated Silver", value: "0.5-1 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Pure Silver", value: "1-2 kg CO₂" },

{ name: "Silver Alloy", value: "1.5-2.5 kg CO₂" },

{ name: "Plated Silver", value: "1.5-2.5 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Pure Silver", value: "4-6 kg CO₂" },

{ name: "Silver Alloy", value: "5-7 kg CO₂" },

{ name: "Plated Silver", value: "5-7 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Pure Silver", value: "2.5-4 kg CO₂" },

{ name: "Silver Alloy", value: "3.5-5 kg CO₂" },

{ name: "Plated Silver", value: "3.5-5 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Pure Silver", value: "1-2 kg CO₂" },

{ name: "Silver Alloy", value: "1.5-2.5 kg CO₂" },

{ name: "Plated Silver", value: "1.5-2.5 kg CO₂" }

]

}

]

},

{

name: 'Namda',

RawMaterial: [

{ name: "Pure Wool", value: "3-4 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "2-3 kg CO₂" },

{ name: "Synthetic Blend", value: "5-6 kg CO₂" }

],

Processing: [

{

name: "Wool Cleaning (Manual)",

values: [

{ name: "Pure Wool", value: "0.5-1 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Blend", value: "0-0 kg CO₂" }

]

},

{

name: "Wool Cleaning (Machine)",

values: [

{ name: "Pure Wool", value: "1-1.5 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "Blending (Manual)",

values: [

{ name: "Pure Wool", value: "0.5-1 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Blend", value: "0-0 kg CO₂" }

]

},

{

name: "Blending (Machine)",

values: [

{ name: "Pure Wool", value: "1-1.5 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand Felting (Simple)",

values: [

{ name: "Pure Wool", value: "2-3 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Blend", value: "3-4 kg CO₂" }

]

},

{

name: "Hand Felting (Intricate)",

values: [

{ name: "Pure Wool", value: "3-4 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Blend", value: "4-5 kg CO₂" }

]

},

{

name: "Machine-Assisted Felting",

values: [

{ name: "Pure Wool", value: "4-5 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "3-4 kg CO₂" },

{ name: "Synthetic Blend", value: "5-6 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Paper/Cloth)",

values: [

{ name: "Pure Wool", value: "0.5-1 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Blend", value: "1-1 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly)",

values: [

{ name: "Pure Wool", value: "1-1.5 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "1.5-2 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Pure Wool", value: "0.5-1 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Blend", value: "1-1.5 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Pure Wool", value: "1-2 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Pure Wool", value: "4-5 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "5-6 kg CO₂" },

{ name: "Synthetic Blend", value: "6-7 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Pure Wool", value: "2.5-4 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "3-4.5 kg CO₂" },

{ name: "Synthetic Blend", value: "4-5.5 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Pure Wool", value: "1-1.5 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

}

]

}

]

},

{

category: 'Sport Crafts',

subcategory: [

{

name: 'Cricket Bat Making',

RawMaterial: [

{ name: "Willow Wood", value: "3-5 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "4-6 kg CO₂" },

{ name: "Synthetic Composite", value: "5-7 kg CO₂" }

],

Processing: [

{

name: "Wood Harvesting (Manual)",

values: [

{ name: "Willow Wood", value: "1-2 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Composite", value: "0-0 kg CO₂" }

]

},

{

name: "Wood Harvesting (Machine)",

values: [

{ name: "Willow Wood", value: "2-3 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Composite", value: "3-4 kg CO₂" }

]

},

{

name: "Handle Assembly (Manual)",

values: [

{ name: "Willow Wood", value: "0.5-1 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "0.5-1.5 kg CO₂" },

{ name: "Synthetic Composite", value: "0-0 kg CO₂" }

]

},

{

name: "Handle Assembly (Machine)",

values: [

{ name: "Willow Wood", value: "1-1.5 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "1-2 kg CO₂" },

{ name: "Synthetic Composite", value: "2-3 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand Shaping (Simple)",

values: [

{ name: "Willow Wood", value: "1-2 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Composite", value: "2-3 kg CO₂" }

]

},

{

name: "Hand Shaping (Intricate)",

values: [

{ name: "Willow Wood", value: "2-3 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Composite", value: "3-4 kg CO₂" }

]

},

{

name: "Machine-Assisted Shaping",

values: [

{ name: "Willow Wood", value: "3-4 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "3-4 kg CO₂" },

{ name: "Synthetic Composite", value: "4-5 kg CO₂" }

]

}

],

Finishing: [

{

name: "Polishing (Manual)",

values: [

{ name: "Willow Wood", value: "0.5-1 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Composite", value: "0-0 kg CO₂" }

]

},

{

name: "Polishing (Machine)",

values: [

{ name: "Willow Wood", value: "1-1.5 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Composite", value: "1.5-2 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Plastic Wrap)",

values: [

{ name: "Willow Wood", value: "0.5-1 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Composite", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly Packaging)",

values: [

{ name: "Willow Wood", value: "1-1.5 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Composite", value: "1.5-2 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Willow Wood", value: "0.5-1 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Composite", value: "1-1.5 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Willow Wood", value: "1-2 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Composite", value: "2-3 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Willow Wood", value: "5-6 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "6-7 kg CO₂" },

{ name: "Synthetic Composite", value: "7-8 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Willow Wood", value: "2-3.5 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "3-4.5 kg CO₂" },

{ name: "Synthetic Composite", value: "4-5.5 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Willow Wood", value: "1-1.5 kg CO₂" },

{ name: "Willow with Synthetic Handle", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Composite", value: "2-3 kg CO₂" }

]

}

]

},

{

name: 'Chess Board Making',

RawMaterial: [

{ name: "Walnut Wood", value: "4-5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "3-4 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "5-6 kg CO₂" }

],

Processing: [

{

name: "Wood Harvesting (Manual)",

values: [

{ name: "Walnut Wood", value: "1-1.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "0-0 kg CO₂" }

]

},

{

name: "Wood Harvesting (Machine)",

values: [

{ name: "Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2-2.5 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "3-4 kg CO₂" }

]

},

{

name: "Base Preparation (Manual)",

values: [

{ name: "Walnut Wood", value: "0.5-1 kg CO₂" },

{ name: "Walnut with MDF Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "0-0 kg CO₂" }

]

},

{

name: "Base Preparation (Machine)",

values: [

{ name: "Walnut Wood", value: "1-1.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "2-3 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand Carving (Simple)",

values: [

{ name: "Walnut Wood", value: "1-2 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "2-3 kg CO₂" }

]

},

{

name: "Hand Carving (Intricate)",

values: [

{ name: "Walnut Wood", value: "2-3 kg CO₂" },

{ name: "Walnut with MDF Base", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "3-4 kg CO₂" }

]

},

{

name: "Machine-Assisted Carving",

values: [

{ name: "Walnut Wood", value: "3-4 kg CO₂" },

{ name: "Walnut with MDF Base", value: "3-4 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "4-5 kg CO₂" }

]

}

],

Finishing: [

{

name: "Polishing (Manual)",

values: [

{ name: "Walnut Wood", value: "0.5-1 kg CO₂" },

{ name: "Walnut with MDF Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "0-0 kg CO₂" }

]

},

{

name: "Polishing (Machine)",

values: [

{ name: "Walnut Wood", value: "1-1.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "1.5-2 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Cardboard)",

values: [

{ name: "Walnut Wood", value: "0.5-1 kg CO₂" },

{ name: "Walnut with MDF Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly Packaging)",

values: [

{ name: "Walnut Wood", value: "1-1.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "1.5-2 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Walnut Wood", value: "0.5-1 kg CO₂" },

{ name: "Walnut with MDF Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "1-1.5 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Walnut Wood", value: "1-2 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "2-3 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Walnut Wood", value: "5-6 kg CO₂" },

{ name: "Walnut with MDF Base", value: "6-7 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "7-8 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Walnut Wood", value: "2.5-3.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "3-4.5 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "4-5.5 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Walnut Wood", value: "1-1.5 kg CO₂" },

{ name: "Walnut with MDF Base", value: "1.5-2 kg CO₂" },

{ name: "Synthetic/Composite Material", value: "2-3 kg CO₂" }

]

}

]

}

]

},

{

category: 'Hide Crafts',

subcategory: [

{

name: 'Leather Craft',

RawMaterial: [

{ name: "Pure Leather", value: "4-6 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "3-5 kg CO₂" },

{ name: "Synthetic Leather", value: "5-7 kg CO₂" }

],

Processing: [

{

name: "Tanning (Vegetable-Based)",

values: [

{ name: "Pure Leather", value: "2-3 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Leather", value: "0-0 kg CO₂" }

]

},

{

name: "Tanning (Chemical-Based)",

values: [

{ name: "Pure Leather", value: "0-0 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "2-3 kg CO₂" },

{ name: "Synthetic Leather", value: "3-4 kg CO₂" }

]

},

{

name: "Dyeing (Natural)",

values: [

{ name: "Pure Leather", value: "0.5-1 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Leather", value: "0-0 kg CO₂" }

]

},

{

name: "Dyeing (Synthetic)",

values: [

{ name: "Pure Leather", value: "0-0 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Leather", value: "2-3 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand Stitching (Simple)",

values: [

{ name: "Pure Leather", value: "1-2 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Leather", value: "2-3 kg CO₂" }

]

},

{

name: "Hand Stitching (Intricate)",

values: [

{ name: "Pure Leather", value: "2-3 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Leather", value: "3-4 kg CO₂" }

]

},

{

name: "Machine-Assisted Stitching",

values: [

{ name: "Pure Leather", value: "3-4 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "3-4 kg CO₂" },

{ name: "Synthetic Leather", value: "4-5 kg CO₂" }

]

}

],

Finishing: [

{

name: "Polishing (Manual)",

values: [

{ name: "Pure Leather", value: "0.5-1 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Leather", value: "0-0 kg CO₂" }

]

},

{

name: "Polishing (Machine)",

values: [

{ name: "Pure Leather", value: "1-1.5 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Leather", value: "1.5-2 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Paper/Cloth)",

values: [

{ name: "Pure Leather", value: "0.5-1 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Leather", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly Packaging)",

values: [

{ name: "Pure Leather", value: "1-1.5 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Leather", value: "1.5-2 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Pure Leather", value: "0.5-1 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Leather", value: "1-1.5 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Pure Leather", value: "1-2 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Leather", value: "2-3 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Pure Leather", value: "5-6 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "6-7 kg CO₂" },

{ name: "Synthetic Leather", value: "7-8 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Pure Leather", value: "2.5-3.5 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "3-4.5 kg CO₂" },

{ name: "Synthetic Leather", value: "4-5.5 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Pure Leather", value: "1-1.5 kg CO₂" },

{ name: "Leather with Synthetic Components", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Leather", value: "2-3 kg CO₂" }

]

}

]

},

{

name: 'Fur Astrakhan Craft',

RawMaterial: [

{ name: "Pure Astrakhan Fur", value: "6-8 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "4-6 kg CO₂" },

{ name: "Synthetic Fur", value: "3-5 kg CO₂" }

],

Processing: [

{

name: "Fur Preparation (Manual)",

values: [

{ name: "Pure Astrakhan Fur", value: "2-3 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Fur", value: "0-0 kg CO₂" }

]

},

{

name: "Fur Preparation (Machine)",

values: [

{ name: "Pure Astrakhan Fur", value: "3-4 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Fur", value: "2-3 kg CO₂" }

]

},

{

name: "Dyeing (Natural)",

values: [

{ name: "Pure Astrakhan Fur", value: "0.5-1 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Fur", value: "0-0 kg CO₂" }

]

},

{

name: "Dyeing (Synthetic)",

values: [

{ name: "Pure Astrakhan Fur", value: "0-0 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Fur", value: "2-3 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand Tailoring (Simple)",

values: [

{ name: "Pure Astrakhan Fur", value: "1-2 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Fur", value: "2-3 kg CO₂" }

]

},

{

name: "Hand Tailoring (Intricate)",

values: [

{ name: "Pure Astrakhan Fur", value: "2-3 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Fur", value: "3-4 kg CO₂" }

]

},

{

name: "Machine-Assisted Tailoring",

values: [

{ name: "Pure Astrakhan Fur", value: "3-4 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "3-4 kg CO₂" },

{ name: "Synthetic Fur", value: "4-5 kg CO₂" }

]

}

],

Finishing: [

{

name: "Polishing (Manual)",

values: [

{ name: "Pure Astrakhan Fur", value: "0.5-1 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Fur", value: "0-0 kg CO₂" }

]

},

{

name: "Polishing (Machine)",

values: [

{ name: "Pure Astrakhan Fur", value: "1-1.5 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Fur", value: "1.5-2 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Paper/Cloth)",

values: [

{ name: "Pure Astrakhan Fur", value: "0.5-1 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Fur", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly Packaging)",

values: [

{ name: "Pure Astrakhan Fur", value: "1-1.5 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Fur", value: "1.5-2 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Pure Astrakhan Fur", value: "0.5-1 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Fur", value: "1-1.5 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Pure Astrakhan Fur", value: "1-2 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Fur", value: "2-3 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Pure Astrakhan Fur", value: "6-7 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "5-6 kg CO₂" },

{ name: "Synthetic Fur", value: "4-5 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Pure Astrakhan Fur", value: "3-4 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Fur", value: "2-3 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Pure Astrakhan Fur", value: "1-1.5 kg CO₂" },

{ name: "Fur-Synthetic Blend", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Fur", value: "1-2 kg CO₂" }

]

}

]

},

]

},

{

category: 'Culinary weaving',

subcategory: [

{

name: 'Wazwan',

RawMaterial: [

{ name: "Local Ingredients", value: "3-4 kg CO₂" },

{ name: "Non-Local Ingredients", value: "5-6 kg CO₂" },

{ name: "Imported Ingredients", value: "7-10 kg CO₂" }

],

Preparation: [

{

name: "Traditional Cooking",

values: [

{ name: "Local Ingredients", value: "2-3 kg CO₂" },

{ name: "Non-Local Ingredients", value: "2.5-4 kg CO₂" },

{ name: "Imported Ingredients", value: "3-5 kg CO₂" }

]

},

{

name: "Modern Cooking",

values: [

{ name: "Local Ingredients", value: "1-2 kg CO₂" },

{ name: "Non-Local Ingredients", value: "1.5-3 kg CO₂" },

{ name: "Imported Ingredients", value: "2-4 kg CO₂" }

]

}

],

CookingProcess: [

{

name: "Cooking Process",

values: [

{ name: "Local Ingredients", value: "2-3 kg CO₂" },

{ name: "Non-Local Ingredients", value: "3-4 kg CO₂" },

{ name: "Imported Ingredients", value: "4-6 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic",

values: [

{ name: "Local Ingredients", value: "0.5-1 kg CO₂" },

{ name: "Non-Local Ingredients", value: "1-1.5 kg CO₂" },

{ name: "Imported Ingredients", value: "1.5-2 kg CO₂" }

]

},

{

name: "Luxury",

values: [

{ name: "Local Ingredients", value: "1-1.5 kg CO₂" },

{ name: "Non-Local Ingredients", value: "1.5-2 kg CO₂" },

{ name: "Imported Ingredients", value: "2-3 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Local Ingredients", value: "0.5-1 kg CO₂" },

{ name: "Non-Local Ingredients", value: "1-1.5 kg CO₂" },

{ name: "Imported Ingredients", value: "1.5-2 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Local Ingredients", value: "1-2 kg CO₂" },

{ name: "Non-Local Ingredients", value: "2-3 kg CO₂" },

{ name: "Imported Ingredients", value: "3-4 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Local Ingredients", value: "5-7 kg CO₂" },

{ name: "Non-Local Ingredients", value: "6-8 kg CO₂" },

{ name: "Imported Ingredients", value: "7-10 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Local Ingredients", value: "1.5-2.5 kg CO₂" },

{ name: "Non-Local Ingredients", value: "2-3 kg CO₂" },

{ name: "Imported Ingredients", value: "3-4 kg CO₂" }

]

}

]

},

{

name: 'Kahwa Pink Tea',

RawMaterial: [

{ name: "Local Ingredients", value: "2-3 kg CO₂" },

{ name: "Non-Local Ingredients", value: "4-5 kg CO₂" },

{ name: "Imported Ingredients", value: "6-8 kg CO₂" }

],

Preparation: [

{

name: "Traditional Brewing",

values: [

{ name: "Local Ingredients", value: "1-2 kg CO₂" },

{ name: "Non-Local Ingredients", value: "1.5-3 kg CO₂" },

{ name: "Imported Ingredients", value: "2-3.5 kg CO₂" }

]

},

{

name: "Modern Brewing (Electric)",

values: [

{ name: "Local Ingredients", value: "0.5-1 kg CO₂" },

{ name: "Non-Local Ingredients", value: "1-1.5 kg CO₂" },

{ name: "Imported Ingredients", value: "1.5-2.5 kg CO₂" }

]

},

{

name: "Additives (Spices, Nuts)",

values: [

{ name: "Local Ingredients", value: "1-1.5 kg CO₂" },

{ name: "Non-Local Ingredients", value: "2-3 kg CO₂" },

{ name: "Imported Ingredients", value: "3-4 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Paper Pouches)",

values: [

{ name: "Local Ingredients", value: "0.5-1 kg CO₂" },

{ name: "Non-Local Ingredients", value: "1-1.5 kg CO₂" },

{ name: "Imported Ingredients", value: "1.5-2 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly Packaging)",

values: [

{ name: "Local Ingredients", value: "1-1.5 kg CO₂" },

{ name: "Non-Local Ingredients", value: "1.5-2 kg CO₂" },

{ name: "Imported Ingredients", value: "2-3 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Local Ingredients", value: "0.5-1 kg CO₂" },

{ name: "Non-Local Ingredients", value: "1-1.5 kg CO₂" },

{ name: "Imported Ingredients", value: "1.5-2 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Local Ingredients", value: "1-2 kg CO₂" },

{ name: "Non-Local Ingredients", value: "2-3 kg CO₂" },

{ name: "Imported Ingredients", value: "3-4 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Local Ingredients", value: "4-5 kg CO₂" },

{ name: "Non-Local Ingredients", value: "5-7 kg CO₂" },

{ name: "Imported Ingredients", value: "6-9 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Local Ingredients", value: "1.5-2.5 kg CO₂" },

{ name: "Non-Local Ingredients", value: "2-3 kg CO₂" },

{ name: "Imported Ingredients", value: "3-4 kg CO₂" }

]

}

]

}

]

},

{

category: 'Recycled Crafts',

subcategory: [

{

name: 'Papier Mache',

RawMaterial: [

{ name: "Recycled Paper Base", value: "2-3 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "3-4 kg CO₂" },

{ name: "Synthetic Base", value: "4-5 kg CO₂" }

],

Processing: [

{

name: "Pulp Preparation (Manual)",

values: [

{ name: "Recycled Paper Base", value: "0.5-1 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Base", value: "0-0 kg CO₂" }

]

},

{

name: "Pulp Preparation (Machine)",

values: [

{ name: "Recycled Paper Base", value: "1-1.5 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Base", value: "2-3 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand Molding (Simple)",

values: [

{ name: "Recycled Paper Base", value: "1-2 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Base", value: "2-3 kg CO₂" }

]

},

{

name: "Hand Molding (Intricate)",

values: [

{ name: "Recycled Paper Base", value: "2-3 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Base", value: "3-4 kg CO₂" }

]

},

{

name: "Machine-Assisted Molding",

values: [

{ name: "Recycled Paper Base", value: "3-4 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "3-4 kg CO₂" },

{ name: "Synthetic Base", value: "4-5 kg CO₂" }

]

}

],

PaintingAndLacquering: [

{

name: "Hand Painting (Simple)",

values: [

{ name: "Recycled Paper Base", value: "1-1.5 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Base", value: "2-2.5 kg CO₂" }

]

},

{

name: "Hand Painting (Intricate)",

values: [

{ name: "Recycled Paper Base", value: "2-3 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Base", value: "3-4 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Paper/Cloth)",

values: [

{ name: "Recycled Paper Base", value: "0.5-1 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Base", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly)",

values: [

{ name: "Recycled Paper Base", value: "1-1.5 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Base", value: "1.5-2 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Recycled Paper Base", value: "0.5-1 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Base", value: "1-1.5 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Recycled Paper Base", value: "1-2 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Base", value: "2-3 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Recycled Paper Base", value: "3-4 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "4-5 kg CO₂" },

{ name: "Synthetic Base", value: "5-6 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Recycled Paper Base", value: "1.5-3 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "2.5-4 kg CO₂" },

{ name: "Synthetic Base", value: "3.5-5 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Recycled Paper Base", value: "1-1.5 kg CO₂" },

{ name: "Recycled Paper with Wood Base", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Base", value: "2-3 kg CO₂" }

]

}

]

},

{

name: 'Gabba',

RawMaterial: [

{ name: "Recycled Wool Base", value: "2-3 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "3-4 kg CO₂" },

{ name: "Synthetic Blend", value: "4-5 kg CO₂" }

],

Processing: [

{

name: "Material Cleaning (Manual)",

values: [

{ name: "Recycled Wool Base", value: "0.5-1 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Blend", value: "0-0 kg CO₂" }

]

},

{

name: "Material Cleaning (Machine)",

values: [

{ name: "Recycled Wool Base", value: "1-1.5 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "Dyeing (Natural)",

values: [

{ name: "Recycled Wool Base", value: "0.5-1 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Blend", value: "0-0 kg CO₂" }

]

},

{

name: "Dyeing (Synthetic)",

values: [

{ name: "Recycled Wool Base", value: "0-0 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

}

],

Crafting: [

{

name: "Hand Stitching (Simple)",

values: [

{ name: "Recycled Wool Base", value: "1-2 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "Hand Stitching (Intricate)",

values: [

{ name: "Recycled Wool Base", value: "2-3 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Blend", value: "3-4 kg CO₂" }

]

},

{

name: "Machine-Assisted Stitching",

values: [

{ name: "Recycled Wool Base", value: "3-4 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "3-4 kg CO₂" },

{ name: "Synthetic Blend", value: "4-5 kg CO₂" }

]

}

],

Embroidery: [

{

name: "Crewel Embroidery (Simple)",

values: [

{ name: "Recycled Wool Base", value: "1-1.5 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Blend", value: "2-2.5 kg CO₂" }

]

},

{

name: "Crewel Embroidery (Intricate)",

values: [

{ name: "Recycled Wool Base", value: "2-3 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "2.5-3.5 kg CO₂" },

{ name: "Synthetic Blend", value: "3-4 kg CO₂" }

]

}

],

Packaging: [

{

name: "Basic (Paper/Cloth)",

values: [

{ name: "Recycled Wool Base", value: "0.5-1 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Blend", value: "1-1.5 kg CO₂" }

]

},

{

name: "Luxury (Eco-Friendly)",

values: [

{ name: "Recycled Wool Base", value: "1-1.5 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "1-1.5 kg CO₂" },

{ name: "Synthetic Blend", value: "1.5-2 kg CO₂" }

]

}

],

Transportation: [

{

name: "Local",

values: [

{ name: "Recycled Wool Base", value: "0.5-1 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "0.5-1 kg CO₂" },

{ name: "Synthetic Blend", value: "1-1.5 kg CO₂" }

]

},

{

name: "Domestic",

values: [

{ name: "Recycled Wool Base", value: "1-2 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "1.5-2.5 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

},

{

name: "International (Air)",

values: [

{ name: "Recycled Wool Base", value: "4-5 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "5-6 kg CO₂" },

{ name: "Synthetic Blend", value: "6-7 kg CO₂" }

]

},

{

name: "International (Sea)",

values: [

{ name: "Recycled Wool Base", value: "2.5-4 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "3-4.5 kg CO₂" },

{ name: "Synthetic Blend", value: "4-5.5 kg CO₂" }

]

},

{

name: "Bulk Shipping (Sea)",

values: [

{ name: "Recycled Wool Base", value: "1-1.5 kg CO₂" },

{ name: "Wool-Cotton Blend", value: "1.5-2 kg CO₂" },

{ name: "Synthetic Blend", value: "2-3 kg CO₂" }

]

}

]

}

]

},

]